****

**CLP2 Series Installation Sheet**

**CLP2-25W-1X4**

**CLP2-25W-2X2**

**CLP2-50W-2X4**

**WARNING:**

**READ CAREFULLY BEFORE INSTALLING FIXTURE. RETAIN THESE INSTRUCTIONS FOR FUTURE REFERENCE.**

**Fixtures must be wired in accordance with the National Electrical Code and all applicable local codes.**

**Risk of fire or electric shock. Flat Panel installation requires knowledge of luminaires electrical systems. If not qualified,**

**do not attempt installation. Contact a qualified electrician. Be certain electrical power is OFF before and during installation and maintenance.**

**Flat Panel must be connected to a wiring system with an equipment – grounding conductor. Make sure the supply voltage is same as the rated luminaire voltage.**

**To prevent wiring damage or abrasion, do not expose wiring to edges of sheet metal or sharp objects.**

**No user serviceable parts inside of Flat Panel.**

**This product is indoor lamps, no waterproof function. Forbid using outdoor or moist places;**

**This product has dimming function, can be used with dimmer**

**Electrical Schematic**



**Recessed Installation**



**Suspension Installation**



www.jdlighting.com

800.749.3920

4 6